OWNERS MANUAL

MODEL:

Condiment Station
condiment dispenser
PART NUMBER:

52001

ASSEMBLY[image: image3.png]



1.
It is suggested that you clean pans and pumps before use. 

2. 
Remove lids from the two pump wells and install pumps.  Unscrew the top of the pump from the bottom. Then insert the bottom of pump through hole in lid and screw the top of pump back into the bottom.

3. 
Freeze cold packs to be ready when needed.  When ready for use lay frozen cold packs in the insulated well and put pans back in place.  Fill pans with desired condiments.

4. 
Insert ketchup and mustard in the correct pump wells and place lid with pump back on top of the well.  The pump will need to be pumped a couple times to pull product to the top of the pump for dispensing. 
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CLEANING THE DISPENSER
1.
The pans and pumps can be washed by hand or in a dishwasher.
2.
The body of the dispenser can be wiped down with a wet cloth inside and out. 
3.
The pumps can be dismantled for easy cleaning.  If you decides to pull the top of the pump off, be careful not to lose small vacuum ball that creates the suction for the pump to work.  For easy cleaning you can pump hot water through the pump to release buildup.
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PARTS LIST

	P/N
	Description

	52011
	chassis

	52012
	Foam insulation kit

	52013
	Ice packs

	52014
	Condiment Lid

	52015
	Hinge set

	52016
	Pump Well Lid

	52017
	Pumps

	52018
	Decal set (red and yellow)


To Order Parts Contact:
Benchmark USA, Inc.
25-J Brookfield Oaks Dr.

Greenville, SC 29607 USA

Tel:  877-432-5500

Fax:  864-312-5505

Email:  parts@benchmarkusainc.com
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Three Year Warranty

THE WARRANTY:

Benchmark USA warrants the original purchaser of new food equipment manufactured by Benchmark USA to be free from defects in material or workmanship from the date of the original purchase for a period of three years.  

WHO IS COVERED BY THIS WARRANTY:

The original purchaser who has provided proper proof of the original retail purchase and all other requested information.

WHAT IS WARRANTIED:

The obligation of Benchmark USA under this warranty is limited to the replacement of any parts or components that in the opinion of Benchmark USA are defective, F.O.B. the factory, or at any other location that Benchmark USA may designate.

WHAT VOIDS THE WARRANTY:

1.  Any piece of equipment that has been installed, operated or maintained inconsistently 

     with Benchmark USA operating instructions.

2.  Any part  or  component  that has been modified, changed or altered from its original 

     configuration.

3.  Any   electrical component   that   has been   damaged due to submergence  in  any   

     liquid.

4.  Any   part   or   component   that   has   been   subject   to abuse, misuse, neglect or 

     accidents.

EXTENT OF WARRANTY:

Any defective component, part or assembly returned to Benchmark USA will be replaced by Benchmark USA.  Benchmark USA will not be responsible for any expenses incurred by the customer under the terms of this warranty, nor shall it be responsible for any damages either consequential, special, contingent, or otherwise; or expenses or injury arising directly or indirectly from the use of a Benchmark USA product.  Any component, part or assembly returned to Benchmark USA must be returned at the customers expense along with proof of purchase.  Benchmark USA reserves the right to determine whether the terms of this warranty have been properly complied with.  In the event that the terms are not complied with, Benchmark USA shall be under no obligation to honor this warranty.    
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